# **Usage:**

Used for lifting, pushing, spreading, bending, pressing, or straightening objects up to 12 tons. Can work in upright, angle or horizontal positions

# **Specifications:**

* Lifting capacity of 5 tons
* Height 9” (Retracted)
* Total extension 18.5”
* Screw extension 3 1/8”
* Ram extension 6”
* Three piece handle 22”

# **safety:**

* Do not exceed load limit.
* Stabilize load before lifting.
* Watch for load weight shift.
* Watch for potential pinch or crushing hazards

# **operations:**

* Connect 3 piece handle
* Close valve by turning clockwise
* Insert handle into hydraulic pump, begin pumping
* To lower place handle on valve, slowly turn counter-clockwise two turns

# **maintenance:**

* Wipe down tool
* Insure tool is functioning properly
* To add or change oil, push ram down remove rubber plug and fill to level of hole with hydraulic jack oil.