# **Usage:**

Used in foam applications when Class A or B foam is needed. Correctly and automatically proportions foam quickly directly from the concentrated foam buckets carried on the apparatus.

# **Specifications:**

**Akron 3095 In-Line Foam Eductor:**

* + Pyrolite construction
	+ Weight: 3½Lbs
	+ Inlet and Outlet Sizes: 1½”
	+ Hose Length: 30”
	+ Flow: 95gpm
	+ Metering Dial: ¼, ½, 1, 3, and 6%
	+ Inlet Operating pressure: 200psi
	+ Nozzle type: Any constant flow from 75 to 100psi

# **other Equipment:**

* Hose
* Foam Concentrate

# **operations:**

* + Remove foam concentrate and foam eductor from apparatus
	+ Attach eductor to outlet/hose
	+ Make sure dial is set to 6%
	+ Place eductor hose in foam concentrate
	+ Call for waterand slay the dragon
	+ Foam application can be banked down, rained on, or rolled onto the fire
	+ When operations are complete flush with fresh water for at least 3min.

# **maintenance:**

* Flush hose and eductor
* Meter dial can be removed for cleaning and inspection

