# **Usage:**

Capable of standard drill or rotary hammer through concrete, steel or wood.

# **Specifications:**

* 24V Battery
* RPM 0-1200
* BPM 0-4400
* Bit Type SDS Plus
* Weight 9.2lbs
* Max Capacity
* -Concrete 7/8”
* -Steel ½”
* -Wood ¾”

# **safety:**

* Do not force tool
* Always use side handle
* Do not use dull or damaged bits
* Ensure bits are secure prior to use
* Be aware of surroundings

# **operations:**

* Make sure tool is in off position
* Depress locking sleeve
* Insert proper bit (make sure bit is locked in)
* Set depth gauge if applicable
* If internal slip clutch engages (bit will bind up) release trigger and reposition tool
* After use remove bit and store tool in stand by position or remove battery

# **maintenance:**

* Rotate battery per weekly battery charging schedule. (Page 78)
* Remove battery, clean tool with compressed dry air
* Wipe down body