# **Usage:**

The Hurst eDraulic Combi-Tool has the capabilities of cutting, spreading, squeezing and pulling combined in one tool.

# **Specifications:**

**Hurst eDraulic Combi SC350E**

* Max. Operating Pressure: 10,500psi
* Max. Cutting Force: 61,600 lbs. @ notch
* Max. Cutting Opening: 14.6”
* Max. Spreading Force:25,400 lbs. @ back of tips
* Max. Spreading Opening: 141/4” @ back of tips
* Weight: 43.7 lbs.

# **operations:**

* Press ON/OFF switch
* Use deadman switch to open and close cutter
* After use leave cutter slightly open
* Wipe down and inspect for damage

# **maintenance:**

* Remove dirt and debris by wiping down
* Use WD-40 to lubricate fittings

