# **irons:**

Manufacturer: various

Description: Flat head married to Halligan Bar

# **Specifications:**

**Halligan**

* Cold rolled or drop forged one piece construction of alloy steel
* 3 feet with pick, adz, and claw

**Flat head axe:**

* 6 or 7 lbs head with 3 foot handle
* 2nd generation hickory handle
* Used as striking tool in conjunction with the Halligan

# **operations:**

* Forcible entry tools used to break glass, make purchase points, force doors, pierce object, sheer lock
* May be used in conjunction with the K-tool for “thru the lock” forcible entry

# **maintenance:**

**Halligan:**

* File burs
* Inspect for chips, dents, cracks, or bends after each use and on Mondays
* Inspect welds

**Flat head axe:**

* Handles should be lightly sanded to remove burs and coated with boiled linseed oil
* Check head for wedge and snugness
* Head should be free of rust and burs
* Sharpen per manufacturer’s specification and coat head with light coat of petroleum lubricate