# **manufacturer:**

Gemtor Inc.

# **Specifications:**

* Pompier Belt is designated as a Class 1 ladder/escape belt
* Regulated by NFPA 1983-2001
* Belt made of specially woven, high strength nylon webbing
* Lock stitched with high tenacity nylon thread
* 3" wide buckle strap.
* 5" wide body pad.
* Double tongue buckle for fast engagement and release of the belt. ~ Zinc plated steel Pompier hook with automatic, one-hand twist
* Lock operation.
* Hardware meets 50-hour salt spray test
* UL classification

# **operations:**

* Required for all aerial ladder operations when working from the ladder
* Once you reach the desired location on the ladder lock the hook to
* The rung for fall protection
* Also designed to be used as an emergency self-rescue device

# **maintenance:**

* Inventory during Wednesday checks, clean and inspect