# **Usage:**

Provides simultaneous two-way communication between Safety Attendant and Entrant/Victim to distances up to 1500 Feet.

# **Specifications:**

* Kit includes 25’ of signal cable w/ twist lock connectors
* Lightweight Headset
* Rescue Probe
* Powered by 4 “AA” Batteries

# **Safety**

Test before putting system into an IDLH atmosphere.Do not change battery in IDLH atmosphere

* Do not put tension on cables
* Check low batter indicator before putting into use.

# **Operations:**

* Switch Power to “On”
* Connect Operator Headset to “Operator Port”
* Switch Mode Selector to “Talk Box” when using Rescue Probe
* Connect signal cable to CSI-1100 and to Rescue Probe
* Set volume
* Test two-way communications

# **maintenance:**

* Check unit at first of the month
* Replace batteries as needed
* Wipe clean if dirty

