# **Usage:**

Used to remove victims in technical rescue situations.

# **Specifications:**

* ASTM Grade 2 Titanium
  + Unalloyed titanium
  + TIG Welded
* Dimensions: 83”x 23”x7.25”
* Weight: 13.5 Lbs.
* Rating: 2,500Lbs
* Double walled head and foot ends
* 1” Tope tube
* Durathene netting won’t corrode, breathes, and won’t snag
* Polyethylene back support
* Fits standard backboard
* Main frame, ribs, skids, inserts
* Solid and Break-down models available

# **operations:**

* Remove from apparatus with backboard
* Attach to rescue system
* Lower with/to rescuer to secure victim
* Lash the patient into basket
* Haul patient and rescuers to safety

# **maintenance:**

* Inspect for cracks, bends and dents that could affect strength
* Inspect netting and back support