# **Usage:**

Ripping and cutting lumber

# **Specifications:**

* Blade Size:
* 1677M 7 ¼”
* 120 volts
* 15 amps
* 5,300 blade RPM

# **Safety:**

* Don’t operate if damage to plug, cord or receptacle.
* Must use eye protection.
* Grip saw firmly.
* Plan cuts prior to cutting.

# **operations:**

* Mark cut line on wood.
* Connect power cord to saw.
* Squeeze trigger and start cut.
* Follow cut line previously marked.

# **maintenance:**

* Wipe down saw after use.
* Inspect blade for chipped teeth.
* Inspect power cord for nicks and plug for bent prongs.

