# **Usage:**

Used as a forcible entry tool to ram, pry, cut, break locks and create openings.

# **Specifications:**

**Pry Axe**

* Heat treated alloy steel
* Chrome plated for easy maintenance
* Steel shaft with press fitted and pinned to the claw
* Rubber sleeve handle
* Weight: 6.6Lbs
* Length: 18”& 28”(extended)
* Pick and Fork
* Serrated Axe
* Optional Metal Cutting Claw

# **operations:**

**To Extend:**

* + Push the release button or the release lever and extend

**To Separate:**

* + Extend the fork to the stop and turn 180o pull and separate
  + 90o prying capabilities

**Ram:**

* + Extend and hold below the shaft with one hand and on the grip with the other and slide to ram.

# **maintenance:**

* Check welds/pins for cracks and separation
* Check for bends
* File to sharpen and remove burs
* Oil shaft