# **Usage:**

We have various types of rope to serve different functions from rescue and life safety applications to hauling tools.

# **Specifications:**

**CMC Life Safety Rescue Rope**


Length: 150’/200’/300’

Diameter: ½” Low Stretch

Less than 5% @ 450LBS

Kernmantle

Material: Nylon

Tensile Strength: 10,000LBS

Working Load: 667LBS

Class 2 Rope

Weight: 7LBS per 100’

Melting Temp.: 435o

**SSP Lifeline-BA Drop Bags**

Length: 50’

Diameter: 3/8” Low Stretch

Kernmantle

Material: Nylon

Tensile Strength: 6,300LBS

Working Load: 420LBS

Class 1 Rope

**Utility Rope Bag**

Length: 100’

Diameter: 1/2”

3 Strand Laid rope

Material: Nylon

# **maintenance:**

**Visually inspect for:**

* Cuts/Abrasion
* Exposed Kern material
* Chemical Exposure
* Imbedded materials

**Feel for:**

* Bumps/Bulges
* Soft spots
* Chemical Exposure
* To clean wash in front loader with cold water and mild detergents
* Hang dry out of sunlight